Some thoughts about the LIFO-DBF:

Under switching topology, LIFO may be changed to communicate observations within a time window, not only the latest one.